{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["sheet1"],"not_rendered":{"charts":0,"images":41,"macros":1,"external_links":0,"defined_names":29,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"sheet1","index":0,"n_rows":293,"n_cols":30,"rows_kept":293,"cut":false,"hidden":false,"merged":[[283,22,283,23],[283,24,283,30],[282,1,282,3],[282,4,282,21],[282,22,282,23],[282,24,282,30],[219,0,220,0],[57,27,58,30],[58,15,58,26],[32,11,32,21],[31,3,31,21],[178,2,178,30],[100,2,100,25],[158,2,158,17],[159,20,159,27],[107,28,107,29],[61,1,61,30],[52,27,52,30],[54,27,54,28],[54,29,54,30],[53,6,53,14],[54,6,54,14],[54,15,54,26],[53,15,53,26],[74,2,74,22],[57,15,57,26],[58,0,58,5],[56,27,56,30],[55,6,58,14],[55,27,55,30],[55,0,55,5],[0,24,0,30],[60,24,60,30],[6,3,6,21],[11,11,11,21],[1,1,1,30],[8,22,8,24],[5,26,5,28],[9,22,9,24],[6,26,6,28],[3,22,3,24],[3,26,3,28],[4,22,4,24],[4,26,4,28],[12,11,12,21],[7,11,7,21],[8,11,8,21],[9,11,9,21],[10,11,10,21],[13,26,13,28],[16,11,16,21],[7,26,7,28],[32,26,32,28],[28,26,28,28],[23,26,23,28],[28,11,28,21],[17,26,17,28],[23,22,23,24],[27,22,27,24],[26,26,26,28],[22,22,22,24],[23,11,23,21],[24,11,24,21],[25,11,25,21],[26,11,26,21],[28,22,28,24],[20,26,20,28],[21,26,21,28],[17,22,17,24],[27,26,27,28],[26,22,26,24],[25,26,25,28],[288,1,288,3],[288,4,288,21],[288,22,288,23],[288,24,288,30],[18,11,18,21],[19,11,19,21],[20,11,20,21],[22,26,22,28],[19,22,19,24],[18,26,18,28],[22,11,22,21],[18,22,18,24],[24,22,24,24],[52,6,52,14],[24,26,24,28],[25,22,25,24],[32,22,32,24],[51,0,51,5],[56,0,56,5],[56,15,56,26],[52,0,52,5],[27,11,27,21],[51,15,51,26],[287,1,287,3],[292,1,292,3],[292,22,292,23],[292,24,292,30],[291,24,291,30],[289,24,289,30],[291,22,291,23],[289,22,289,23],[291,1,291,3],[289,1,289,3],[289,4,289,21],[291,4,291,21],[292,4,292,21],[290,1,290,3],[290,4,290,21],[290,22,290,23],[290,24,290,30],[287,4,287,21],[287,22,287,23],[287,24,287,30],[286,1,286,3],[286,4,286,21],[286,22,286,23],[286,24,286,30],[54,0,54,5],[51,6,51,14],[53,0,53,5],[51,27,51,30],[52,15,52,26],[57,0,57,5],[55,15,55,26],[285,1,285,3],[285,4,285,21],[285,22,285,23],[285,24,285,30],[284,1,284,3],[284,4,284,21],[284,22,284,23],[284,24,284,30],[283,1,283,3],[283,4,283,21],[3,3,3,21],[21,11,21,21],[20,22,20,24],[19,26,19,28],[21,22,21,24],[7,22,7,24],[13,11,13,21],[13,22,13,24],[11,22,11,24],[8,26,8,28],[11,26,11,28],[10,26,10,28],[15,3,15,21],[17,11,17,21],[12,22,12,24],[9,26,9,28],[10,22,10,24],[14,26,14,28],[16,26,16,28],[16,22,16,24],[12,26,12,28]]}
[]
[null,"Ordering data for on-load tap-changer type (V)UC"]
["Table of"]
["contents",null,null,"END CUSTOMER, COUNTRY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Section",null,null,null,"Page.No"]
[null,null,null,null,null,null,null,null,null,null,null,"End Customer, Country",null,null,null,null,null,null,null,null,null,null,"CC",null,null,null,2]
[]
[null,null,null,"TRANSFORMER DATA (AA-AJ)"]
[null,null,null,null,null,null,null,null,null,null,null,"Type",null,null,null,null,null,null,null,null,null,null,"AA",null,null,null,2]
[null,null,null,null,null,null,null,null,null,null,null,"Rated power",null,null,null,null,null,null,null,null,null,null,"AB",null,null,null,2]
[null,null,null,null,null,null,null,null,null,null,null,"Electric data",null,null,null,null,null,null,null,null,null,null,"AC",null,null,null,2]
[null,null,null,null,null,null,null,null,null,null,null,"OLTC is placed ",null,null,null,null,null,null,null,null,null,null,"AD",null,null,null,2]
[null,null,null,null,null,null,null,null,null,null,null,"OLTC insulation level",null,null,null,null,null,null,null,null,null,null,"AE",null,null,null,3]
[null,null,null,null,null,null,null,null,null,null,null,"Type of switching",null,null,null,null,null,null,null,null,null,null,"AG",null,null,null,3]
[null,null,null,null,null,null,null,null,null,null,null,"General",null,null,null,null,null,null,null,null,null,null,"AJ",null,null,null,3]
[]
[null,null,null,"ON-LOAD TAP-CHANGER DATA (BA-BX)"]
[null,null,null,null,null,null,null,null,null,null,null,"OLTC type designation",null,null,null,null,null,null,null,null,null,null,"BA",null,null,null,3]
[null,null,null,null,null,null,null,null,null,null,null,"Electrical data",null,null,null,null,null,null,null,null,null,null,"BC",null,null,null,3]
[null,null,null,null,null,null,null,null,null,null,null,"Overload requirements",null,null,null,null,null,null,null,null,null,null,"BF",null,null,null,3]
[null,null,null,null,null,null,null,null,null,null,null,"Position of motor-drive",null,null,null,null,null,null,null,null,null,null,"BG",null,null,null,4]
[null,null,null,null,null,null,null,null,null,null,null,"Effective number of turns",null,null,null,null,null,null,null,null,null,null,"BH",null,null,null,4]
[null,null,null,null,null,null,null,null,null,null,null,"Short circuit current",null,null,null,null,null,null,null,null,null,null,"BJ",null,null,null,4]
[null,null,null,null,null,null,null,null,null,null,null,"Language for rating plate",null,null,null,null,null,null,null,null,null,null,"BK",null,null,null,4]
[null,null,null,null,null,null,null,null,null,null,null,"Tie-in resistor",null,null,null,null,null,null,null,null,null,null,"BL",null,null,null,5]
[null,null,null,null,null,null,null,null,null,null,null,"Surface treatment",null,null,null,null,null,null,null,null,null,null,"BN",null,null,null,5]
[null,null,null,null,null,null,null,null,null,null,null,"Top section",null,null,null,null,null,null,null,null,null,null,"BO",null,null,null,5]
[null,null,null,null,null,null,null,null,null,null,null,"Supervisory devices",null,null,null,null,null,null,null,null,null,null,"BT",null,null,null,6]
[null,null,null,null,null,null,null,null,null,null,null,"Oil filter unit",null,null,null,null,null,null,null,null,null,null,"BU",null,null,null,6]
[null,null,null,null,null,null,null,null,null,null,null,"Drain valve",null,null,null,null,null,null,null,null,null,null,"BX",null,null,null,6]
[]
[]
[null,null,null,"OTHER (FR)"]
[null,null,null,null,null,null,null,null,null,null,null,"Further req. and revision spec.",null,null,null,null,null,null,null,null,null,null,"FR1",null,null,null,7]
[]
[]
[]
[null,null,null,"Filled marking ",null,null,null,null,"means non std"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["auth./Prep.",null,null,null,null,null,"Final customer and country",null,null,null,null,null,null,null,null,"Title",null,null,null,null,null,null,null,null,null,null,null,"Date/Appr."]
[null,null,null,null,null,null," "]
["auth./Prep.",null,null,null,null,null,"Company (Buyer of the OLTC)",null,null,null,null,null,null,null,null,"Doc.kind",null,null,null,null,null,null,null,null,null,null,null,"Page",null,"Cont"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,2]
["Dep.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Order No.",null,null,null,null,null,null,null,null,null,null,null,"Lang"]
[]
["Rev.id.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Doc.id."]
[]
[]
[]
["Section","Ordering data for on-load tap-changer type (V)UC"]
["CC"]
[null,null,null,"Order",null,null,null,"Inquiry"]
[]
[null,null,"End Customer",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Country"]
[]
["AA"]
["Type of",null,null,"Network",null,null,null,null,null,null,null,null,"Rectifier / Converter",null,null,null,null,null,null,null,null,"Other (additional info needed in"]
["transformer",null,null,"Generator step-up (GSU)",null,null,null,null,null,null,null,null,"Shunt reactor",null,null,null,null,null,null,null,null,null,null,"further requirements)"]
["application",null,null,"Arc Furnace",null,null,null,null,null,null,null,null,"Phase shifting transformer"]
[null,null,"Transformer with Booster",null,null,null,null,null,null,null,null,"No",null,null,"Yes"]
[null,null,null,"3-phase",null,null,null,null,"1-phase (of 3-phase bank)",null,null,null,null,null,null,null,null,null,"1-phase (solitary)"]
[]
["AB",null,"Note: In case of a single phase unit of a 3-phase bank, state the 3-phase power"]
["Rated power",null,"Rated power ",null,null,null,null,null,null,null,null,null,"MVA"]
[]
["AC"]
["Electric data",null,"System voltage (HV /LV)",null,null,null,null,null,null,null,null,null,"/",null,null,null,"kV",null,"Frequency",null,null,null,null,null,null,"Hz"]
[]
[null,null,"Regulating range: +/-",null,null,null,null,null,null,null,null,null,"/",null,null,null,"x",null,null,null,"% of"]
[]
[null,null,null,"HV winding",null,null,null,null,"LV winding"]
[]
[null,null,"Connections (HV):",null,null,null,null,null,null,"Y",null,"D",null,null,"Connections (LV):",null,null,null,null,null,null,"Y",null,"D"]
[]
[null,null,null,"Auto LV regulated (CFVV)",null,null,null,null,null,null,null,null,"Auto HV regulated (CFVV)",null,null,null,null,null,null,null,null,"Auto Flux regulated (VFVV)"]
[]
["AD"]
["OLTC is",null,null,"Neutral point",null,null,null,null,null,null,"Middle",null,null,null,null,null,null,"Line end single",null,null,null,null,null,null,"Middle single"]
["placed"]
["in the"]
[]
[]
[null,null,null,"Line end 3 phase (B)",null,null,null,null,null,null,"Line end 3 phase (T)",null,null,null,null,null,null,"Middle 3 phase (T)"]
[]
[]
[]
[]
[null,null,"of the:",null,null,"HV winding",null,null,null,null,null,"LV winding"]
["AE"]
["OLTC",null,"Note: Fill in your calculated values for LI-AC.",null,null,null,null,null,null,null,null,null,null,null,null,"For distances, see section AG or Technical Guide."]
["insultaion",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LI",null,null,null,"AC"]
["level",null,"Insulation level to earth g1",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",null,null,null,"kV"]
[]
[null,null,"Between open contacts in diverter switch b2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",null,null,null,"kV"]
[]
[null,null,"Between open contacts in diverter switch e1",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",null,null,null,"kV"]
[]
[null,null,"Between phases b1",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",null,null,null,"kV"]
[]
[null,null,"Between phases d1",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",null,null,null,"kV"]
[]
[null,null,"Across regulating winding a2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",null,null,null,"kV"]
[]
[null,null,"Across regulating winding c1",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",null,null,null,"kV"]
[]
["AG"]
["Type of ",null,null,"Linear",null,null,null,null,"Plus / Minus",null,null,null,null,"Coarse / Fine",null,null,null,null,"Specify the leakage inductance through the"]
["switching",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"coarse and fine windings in series (L)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"(only for Coarse / Fine)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"mH"]
[]
[]
[]
[]
["AJ"]
["General",null,"Type of insulation medium",null,null,null,null,null,null,null,null,"Mineral oil",null,null,null,null,"Other (additional info needed in further req.)"]
[]
["BA",null,"(According to Technical Guide)"]
["OLTC type",null,"Type",null,null,"UCG",null,null,null,"VUCG",null,null,null,"UCL",null,null,null,"VUCL",null,null,null,"UCC",null,null,null,"UCD"]
["designation"]
[null,null,"Insulation level",null,null,null,null,null,null,null,null,null,"Max rated through current"]
[]
[null,null,"Short version",null,null,null,null,null,"No",null,"Yes",null,"Tap Selector type",null,null,null,null,null,null,"C",null,null,"III",null,null,"IV"]
[]
["BC"]
["Electr. Data",null,"Number of electrical positions: "]
[]
[null,null,"Rated phase step voltage:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"V"]
[]
[null,null,"Rated through current ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
[null,null,"(=max phase current in the OLTC winding)"]
["BF"]
["Overload",null,"According to",null,null,null,null,"IEC 60076-7 / IEEE C57.91-2011",null,null,null,null,null,null,null,null,null,null,"Other overload requirement"]
["requirements",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"(additional info needed in further req.)"]
["BG"]
["Position of ",null,"Compare Technical Guide regarding lengths L1, L2, L3, L4",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," α ="]
["motor-drive"]
[]
[]
[null,null,null,"500 < L1 <= 1700",null,null,null,null,null,null,null,"1700 < L1 <= 3200",null,null,null,null,null,null,null,null,"Special shaft system on request"]
[null,null,null,"525 < L2 <= 1800",null,null,null,null,null,null,null,"1800 < L2 <= 3300"]
[null,null,null,"500 < L3<= 1700",null,null,null,null,null,null,null,"1700 < L3 <= 3200"]
[null,null,null,"500 < L4<= 1700",null,null,null,null,null,null,null,"1700 < L4 <= 3200"]
[]
["BH",null,"Note: Marking of mechanical position indicator. The below figures shows the OLTC in the two end positions. "]
["Effective ",null,"State the designations for the end position connecting max turns and the end position connecting min turns. "]
["number of",null,"Three standard alternatives: ( 1 .. N) (Ln .. N .. Rn) (-n .. 0 .. +n)  "]
["turns",null,null,null,null,"Linear",null,null,null,null,null,null,"Plus/minus",null,null,null,null,null,null,null,"Coarse/fine"]
[]
[]
[]
[]
[]
[null,null,"Pos named"]
[null,null,null,null,null,null,"A raise command means operation towards position [ ]."]
[]
["BJ"]
["Short circuit",null,"RMS value (2ms): ",null,null,null,null,null,null,null,"kA",null,"RMS value (3ms): ",null,null,null,null,null,null,null,"kA",null,"Peak value: ",null,null,null,null,null,null,"kA"]
["current"]
["BK"]
["Language for",null,null,"Chinese",null,null,null,null,"English",null,null,null,null,"Greek",null,null,null,null,"Portuguese",null,null,null,null,"Swedish"]
["rating plate",null,null,"Croatian",null,null,null,null,"Estonian",null,null,null,null,"Italian",null,null,null,null,"Romanian",null,null,null,null,"Turkish"]
[null,null,null,"Czech",null,null,null,null,"Finnish",null,null,null,null,"Latvian",null,null,null,null,"Russian",null,null,null,null,"Other"]
[null,null,null,"Danish",null,null,null,null,"French",null,null,null,null,"Norwegian",null,null,null,null,"Slovak",null,null,null,"(additional info needed in "]
[null,null,null,"Dutch",null,null,null,null,"German",null,null,null,null,"Polish",null,null,null,null,"Spanish",null,null,null,"further req.)"]
["BL"]
["Tie-in resistor",null,"Tie-in resistor. Needed only if recovery voltage of the change-over selector exceeds 35 kV"]
[null,null,"Values below needs to be filled both for standard / non standard."]
[null,null,null,"No",null,null,"Std",null,"(As Pre-calculated)"]
[]
[null,null,null,"To be calculated by SECOM / Order Design"]
[]
[null,null,"Note:",null,"With other arrangement than figures below, remember to attach winding layout, winding connections"]
[null,null,null,null,"and capacitances between windings in order to get  tie-in resistance calculated by ABB"]
[null,null,null,null,null,null,"Capacit. C1 (nF)",null,null,null,null,null,null,null,null,null,null,null,null,"Capacit. C2 (nF)"]
[null,null,null,null,null,null,"Regulating winding is placed:"]
[null,null,null,null,null,null,null,"Between winding ",null,null,null,null,null,null,"Between winding ",null,null,null,null,null,null,"Between two"]
[null,null,null,null,null,null,null,"and wall",null,null,null,null,null,null,"and core",null,null,null,null,null,null,"windings"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,"HV",null,null,null,null,null,null,"HV",null,null,null,null,null,null,"HV",null,null,null,null,"HV"]
[null,null,null,null,null,null,null,"LV",null,null,null,null,null,null,"LV",null,null,null,null,null,null,"LV",null,null,null,null,"LV"]
[null,null,null,null,null,null,null,"Other winding",null,null,null,null,null,null,"Other winding",null,null,null,null,null,null,"Other winding",null,null,null,null,"Other winding"]
[null,null,null,null,null,null,null,null,null,"kV",null,null,null,null,null,null,"kV",null,null,null,null,null,null,"kV",null,null,null,null,"kV"]
[]
[null,null,null,null,null,null,null,"Y",null,"D",null,null,null,null,"Y",null,"D",null,null,null,null,"Y",null,"D",null,null,"Y",null,"D"]
[null,null,null,null,null,null,"Place for tie-in resistor"]
[null,null,null,null,null,null,null,"Mounted under the tap selector (not available when using tie-in resistor switch)"]
[null,null,null,null,null,null,null,"Stand alone at optional place in the transformer tank"]
[null,null,null,null,null,null,"Switch for tie-in resistor (Not available for tap-selector type C)"]
[null,null,null,null,null,null,null,"No",null,null,"Yes"]
[]
["BN",null,"Note: Environmental class C3 according to ISO/DIS 12944 for color Munsell 5.5B 5.5/1.25"]
["Surface",null,null,"C3",null,null,"C4",null,null,"C5 M H",null,null,null,"Other"]
["treatment"]
[null,null,"Colour"]
[]
["BO"]
["Top section",null,null,"Cover mounting",null,null,null,null,null,"Yoke mounting on transformer's active part (Needed for bell type transformer)"]
[]
[]
[]
[]
[]
["BT"]
["Supervisory devices",null,"Vertical distance H between the pressure relay device ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"m"]
[null,null,"and the oil level in the conservator"]
[null,null,"Note: One-way breather influences the set point level of our safety devices. "]
[null,null,"Add 4m to the real distance H if one-way breather is used."]
[]
[null,null,"Note: Pressure relay and/or oil flow relay must be choosen."]
[null,null,"Pressure relay",null,null,null,null,null,null,null,null,null,"No",null,null,"Yes, double contacts"]
[null,null,"Oil flow relay",null,null,null,null,null,null,null,null,null,"No",null,null,"One NO + One NO/NC",null,null,null,null,null,null,null,"Two NO"]
[null,null,"Pressure relief device",null,null,null,null,null,null,null,null,null,"No",null,null,"50 mm, double contacts",null,null,null,null,null,null,null,"130 mm, double contacts"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Prepared for 50 mm",null,null,null,null,null,null,null,"Prepared for 130 mm"]
[null,null,"Temperature relay",null,null,null,null,null,null,null,null,null,"No",null,null,"+115 degrees C",null,null,null,null,null,null,null,null,"-25 degrees C"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"+105 degrees C",null,null,null,null,null,null,null,null,"-40 degrees C"]
[null,null,"Temperature sensor PT100 ",null,null,null,null,null,null,null,null,null,"No",null,null,"Yes"]
[null,null,"(Needed for TEC)"]
[]
["BU"]
["Oil filter unit",null,null,"No",null,null,"Yes",null,"Note: Not in combination with temperature relay"]
[]
[null,null,"Voltage for motor:",null,null,null,null,null,"3~ 50 Hz 220-250 V",null,null,null,null,null,null,"3~ 60 Hz 208-277 V",null,null,null,null,null,null,"1~ 50/60 Hz 110-127 V"]
[null,null,null,null,null,null,null,null,"3~ 50 Hz 380-433 V",null,null,null,null,null,null,"3~ 60 Hz 360-480 V",null,null,null,null,null,null,"1~ 50/60 Hz 220-240 V"]
[null,null,null,null,null,null,null,null,"3~ 50 Hz 500 V"]
[]
["BX"]
["Drain & oil",null,null,"No, only cover",null,null,null,null,null,"R1\" inside thread"]
["sampling",null,null,null,null,null,null,null,null,"R1\" outside thread"]
["valve",null,null,null,null,null,null,null,null,"NPT1\" inside thread"]
[null,null,null,null,null,null,null,null,null,"With flange for oil filter unit"]
["FR1",null,"All extras must be noted!"]
["Further "]
["requirements"]
["and revision"]
["specifications"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Section",null,null,"Amendments",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Date",null,"Name"]