{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":35,"macros":1,"external_links":0,"defined_names":27,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":232,"n_cols":30,"rows_kept":232,"cut":false,"hidden":false,"merged":[[23,26,23,28],[24,26,24,28],[57,27,57,30],[53,27,53,28],[53,29,53,30],[26,26,26,28],[50,27,50,30],[52,15,52,26],[56,27,56,30],[55,27,55,30],[57,15,57,26],[50,15,50,26],[54,15,54,26],[56,15,56,26],[51,15,51,26],[53,15,53,26],[10,26,10,28],[13,22,13,24],[16,11,16,21],[17,11,17,21],[9,11,9,21],[10,11,10,21],[13,11,13,21],[11,11,11,21],[12,11,12,21],[11,22,11,24],[12,22,12,24],[11,26,11,28],[12,26,12,28],[6,26,6,28],[7,22,7,24],[7,26,7,28],[9,22,9,24],[9,26,9,28],[203,0,204,0],[144,2,144,17],[0,24,0,30],[59,24,59,30],[51,27,51,30],[56,0,56,5],[54,27,54,30],[54,0,54,5],[55,0,55,5],[55,15,55,26],[8,22,8,24],[8,26,8,28],[6,3,6,21],[7,11,7,21],[1,1,1,30],[6,22,6,24],[222,2,222,28],[164,2,164,29],[22,26,22,28],[25,26,25,28],[57,0,57,5],[54,6,57,14],[61,1,61,15],[60,1,60,30],[61,16,61,30],[51,6,51,14],[50,0,50,5],[50,6,50,14],[87,2,87,5],[52,0,52,5],[29,26,29,28],[30,26,30,28],[8,11,8,21],[74,2,74,22],[29,22,29,24],[25,22,25,24],[24,22,24,24],[23,22,23,24],[22,22,22,24],[30,22,30,24],[10,22,10,24],[52,6,52,14],[53,0,53,5],[53,6,53,14],[51,0,51,5],[21,22,21,24],[18,22,18,24],[26,22,26,24],[18,26,18,28],[19,26,19,28],[13,26,13,28],[21,26,21,28],[20,22,20,24],[16,22,16,24],[16,26,16,28],[17,22,17,24],[17,26,17,28],[19,22,19,24],[20,26,20,28],[3,3,3,21],[3,22,3,24],[3,26,3,28],[4,22,4,24],[4,26,4,28]]}
[]
[null,"Ordering data for on-load tap-changer type VUBB"]
["Table of"]
["contents",null,null,"END CUSTOMER, COUNTRY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Section",null,null,null,"Page.No"]
[null,null,null,null,null,null,null,null,null,null,null,"End Customer, Country",null,null,null,null,null,null,null,null,null,null,"CC",null,null,null,2]
[]
[null,null,null,"TRANSFORMER DATA (AA-AH)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Section",null,null,null,"Page.No"]
[null,null,null,null,null,null,null,null,null,null,null,"Type",null,null,null,null,null,null,null,null,null,null,"AA",null,null,null,2]
[null,null,null,null,null,null,null,null,null,null,null,"Rated power",null,null,null,null,null,null,null,null,null,null,"AB",null,null,null,2]
[null,null,null,null,null,null,null,null,null,null,null,"Electric data",null,null,null,null,null,null,null,null,null,null,"AC",null,null,null,2]
[null,null,null,null,null,null,null,null,null,null,null,"OLTC is placed",null,null,null,null,null,null,null,null,null,null,"AD",null,null,null,2]
[null,null,null,null,null,null,null,null,null,null,null,"OLTC insulation level",null,null,null,null,null,null,null,null,null,null,"AE",null,null,null,2]
[null,null,null,null,null,null,null,null,null,null,null,"Type of switching",null,null,null,null,null,null,null,null,null,null,"AG",null,null,null,3]
[null,null,null,null,null,null,null,null,null,null,null,"General",null,null,null,null,null,null,null,null,null,null,"AJ",null,null,null,3]
[]
[null,null,null,"ON-LOAD TAP-CHANGER DATA (BA-BZ)"]
[null,null,null,null,null,null,null,null,null,null,null,"OLTC type designation",null,null,null,null,null,null,null,null,null,null,"BA",null,null,null,3]
[null,null,null,null,null,null,null,null,null,null,null,"Electrical data",null,null,null,null,null,null,null,null,null,null,"BC",null,null,null,3]
[null,null,null,null,null,null,null,null,null,null,null,"Overload requirements",null,null,null,null,null,null,null,null,null,null,"BF",null,null,null,3]
[null,null,null,null,null,null,null,null,null,null,null,"Position of motor-drive",null,null,null,null,null,null,null,null,null,null,"BG",null,null,null,3]
[null,null,null,null,null,null,null,null,null,null,null,"Effective number of turns",null,null,null,null,null,null,null,null,null,null,"BH",null,null,null,3]
[null,null,null,null,null,null,null,null,null,null,null,"Short circuit current",null,null,null,null,null,null,null,null,null,null,"BJ",null,null,null,4]
[null,null,null,null,null,null,null,null,null,null,null,"Language for rating plate",null,null,null,null,null,null,null,null,null,null,"BK",null,null,null,4]
[null,null,null,null,null,null,null,null,null,null,null,"Tie-in resistor",null,null,null,null,null,null,null,null,null,null,"BL",null,null,null,4]
[null,null,null,null,null,null,null,null,null,null,null,"Surface treatment",null,null,null,null,null,null,null,null,null,null,"BN",null,null,null,4]
[null,null,null,null,null,null,null,null,null,null,null,"Top section",null,null,null,null,null,null,null,null,null,null,"BO",null,null,null,5]
[null,null,null,null,null,null,null,null,null,null,null,"Supervisory devices",null,null,null,null,null,null,null,null,null,null,"BT",null,null,null,5]
[]
[null,null,null,"OTHER (FRQ)"]
[null,null,null,"",null,null,null,null,null,null,null,"Documents",null,null,null,null,null,null,null,null,null,null,"DA",null,null,null,5]
[null,null,null,null,null,null,null,null,null,null,null,"Further req. and revision spec.",null,null,null,null,null,null,null,null,null,null,"FR1",null,null,null,6]
[]
[]
[]
[null,null,null,"Filled marking ",null,null,null,null,"means non std"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Auth./Prep.",null,null,null,null,null,"Final customer and country",null,null,null,null,null,null,null,null,"Title",null,null,null,null,null,null,null,null,null,null,null,"Date/Appr."]
[" "]
["App.",null,null,null,null,null,"Company (Buyer of the OLTC)",null,null,null,null,null,null,null,null,"Doc.kind",null,null,null,null,null,null,null,null,null,null,null,"Page",null,"Cont"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,2]
["Dep.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Order No",null,null,null,null,null,null,null,null,null,null,null,"Lang"]
[]
["Rev.id.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Doc.id."]
[]
[]
[]
[null,"Ordering data for on-load tap-changer type VUBB"]
["Section"]
["CC"]
[null,null,null,"Order",null,null,null,"Inquiry"]
[]
[null,null,"End Customer",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Country"]
[]
["AA"]
["Type",null,null,"Network"]
[null,null,null,"Generator step-up (GSU)"]
[null,null,null,"Other (additional info needed in further requirements)"]
[null,null,"Transformer with Booster",null,null,null,null,null,null,null,null,"No",null,null,"Yes"]
[null,null,null,"3-phase",null,null,null,"1-phase (solitary)"]
[]
["AB"]
["Rated power",null,"Rated power ",null,null,null,null,null,null,null,null,"MVA"]
[]
["AC"]
["Electric data",null,"System Voltage (HV / LV):",null,null,null,null,null,null,null,null,null,null,"  /",null,null,null," kV",null,"Frequency",null,null,null,null,null,null,"Hz"]
[null,null,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,"Regulating range: +/-",null,null,null,null,null,null,null,null,null,null,"/",null,null,null,"x",null,null,null,"    % of"]
[]
[null,null,null,"HV winding",null,null,null,null,"LV winding"]
[]
[null,null,"Connections (HV):",null,null,null,null,null,null,"Y",null,"D",null,null,"Connections (LV):",null,null,null,null,null,null,"Y",null,"D"]
[]
[null,null,null,"Auto LV regulated (CFVV)",null,null,null,null,null,null,null,null,"Auto HV regulated (CFVV)",null,null,null,null,null,null,null,null,"Auto Flux regulated (VFVV)"]
[]
["AD"]
["OLTC is",null,null,"Neutral point",null,null,null,null,null,null,"Middle",null,null,null,null,null,null,"Line end single",null,null,null,null,null,null,"Middle single"]
["placed"]
["in the"]
[]
[]
[]
[null,null,"of the:",null,null,"HV winding",null,null,null,null,"LV winding"]
[]
["AE"]
["OLTC",null,"Note: Fill in your calculated values for LI-AC.",null,null,null,null,null,null,null,null,null,null,null,null,"For distances, see section AG or Technical Guide."]
["insulation",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LI",null,null,null,"AC"]
["level",null,"Insulation level to earth g2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",null,null,null,"kV"]
[]
[null,null,"Between phases b1",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",null,null,null,"kV"]
[]
[null,null,"Between phases d1",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",null,null,null,"kV"]
[]
[null,null,"Across regulating winding a2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",null,null,null,"kV"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
["AG"]
["Type of ",null,null,"Linear",null,null,null,null,"Plus / Minus",null,null,null,null,"Coarse / Fine",null,null,null,null,"Specify the leakage inductance through the"]
["switching",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"coarse and fine windings in series (L)"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"mH"]
[]
[]
[]
[]
["AJ"]
["General",null,"Type of insulation medium",null,null,null,null,null,null,null,null,"Mineral oil",null,null,null,null,"Other (additional info needed in further req.)"]
[null,null,"Caps",null,null,null,null,null,null,null,null,"No",null,null,null,null,"Yes"]
[]
["BA"]
["OLTC type",null,"Type",null,null,null,null,null,null,null,null,"VUBB",null,"(According to Technical Guide)"]
["designation",null,"Insulation level",null,null,null,null,null,null,null,null,"200",null,null,"380"]
[null,null,"Max rated through current",null,null,null,null,null,null,null,null,"250",null,null,"400",null,null,"600"]
[]
["BC"]
["Electr. Data",null,"Number of electrical positions: "]
[]
[null,null,"Rated phase step voltage:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"V"]
[]
[null,null,"Rated through current ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
[null,null,"(=max phase current in the OLTC winding)"]
["BF"]
["Overload",null,"According to",null,null,null,null,"IEC 60076-7 / IEEE C57.91-2011",null,null,null,null,null,null,null,null,null,null,"Other overload requirement"]
["requirements",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"(additional info needed in further req.)"]
["BG"]
["Position of ",null,"Compare Technical Guide regarding lengths L1, L2"]
[]
["motor-drive",null,null,"500 < L1 <= 1700",null,null,null,null,null,null,"1700 < L1 <= 3200"]
[null,null,null,"525 < L2 <= 1800",null,null,null,null,null,null,"1800 < L2 <= 3300",null,null,null,null,null,null,null,null,null,null,null,null,""]
[]
["BH",null,"Note: Marking of mechanical position indicator. The below figures shows the OLTC in the two end positions. "]
["(See also CF)",null,"State the designations for the end position connecting max turns and the end position connecting min turns. "]
["Effective ",null,"Three standard alternatives: ( 1 .. N) (Ln .. N .. Rn) (-n .. 0 .. +n)  "]
["number of",null,null,null,null,"Linear",null,null,null,null,null,null,"Plus/Minus",null,null,null,null,null,null,null,"Coarse/Fine"]
["turns"]
[]
[]
[]
[]
[null,null,"Pos named"]
[]
["BJ"]
["Short circuit",null,null,"Rms value max 6 kA, 3 s"]
["current",null,null,"Peak value max 15 kA"]
[]
["BK"]
["Language",null,null,"Chinese",null,null,null,null,"English",null,null,null,null,"Greek",null,null,null,null,"Portuguese",null,null,null,null,"Swedish"]
["for rating ",null,null,"Croatian",null,null,null,null,"Estonian",null,null,null,null,"Italian",null,null,null,null,"Romanian",null,null,null,null,"Turkish"]
["plate",null,null,"Czech",null,null,null,null,"Finnish",null,null,null,null,"Latvian",null,null,null,null,"Russian",null,null,null,null,"Other"]
[null,null,null,"Danish",null,null,null,null,"French",null,null,null,null,"Norwegian",null,null,null,null,"Slovak",null,null,null,"(additional info needed in "]
[null,null,null,"Dutch",null,null,null,null,"German",null,null,null,null,"Polish",null,null,null,null,"Spanish",null,null,null,"further req.)"]
[]
["BL"]
["Tie-in resistor",null,"Tie-in resistor.  Needed only if recovery voltage of the change-over selector exceeds 40 kV"]
[null,null,null,"No",null,null,"Std",null,"(As Pre-calculated)"]
[]
[null,null,null,"To be calculated by SECOM or Order Design"]
[null,null,"Note:",null,"With other arrangement than figures below, remember to attach winding layout, winding connections"]
[null,null,null,null,"and capacitances between windings in order to get  tie-in resistance calculated by ABB"]
[null,null,null,null,null,"Capacit. C1 (nF)",null,null,null,null,null,null,null,null,null,null,null,null,"Capacit. C2 (nF)"]
[null,null,null,null,null,"Regulating winding is placed:"]
[null,null,null,null,null,null,"Between winding ",null,null,null,null,null,null,"Between winding ",null,null,null,null,null,null,"Between two"]
[null,null,null,null,null,null,"and wall",null,null,null,null,null,null,"and core",null,null,null,null,null,null,"windings"]
[]
[]
[]
[]
[null,null,null,null,null,null,"HV",null,null,null,null,null,null,"HV",null,null,null,null,null,null,"HV",null,null,null,null,"HV"]
[null,null,null,null,null,null,"LV",null,null,null,null,null,null,"LV",null,null,null,null,null,null,"LV",null,null,null,null,"LV"]
[null,null,null,null,null,null,"Other winding",null,null,null,null,null,null,"Other winding",null,null,null,null,null,null,"Other winding",null,null,null,null,"Other winding"]
[null,null,null,null,null,null,null,null,"kV",null,null,null,null,null,null,"kV",null,null,null,null,null,null,"kV",null,null,null,null,"kV"]
[null,null,null,null,null,null,null,"Y","D",null,null,null,null,null,"Y","D",null,null,null,null,null,"Y","D",null,null,null,"Y","D"]
[null,null,null,null,null,"Tie in resistor will be placed stand alone in transformer tank"]
[null,null,null,null,null,"Switch for tie in resistor"]
[null,null,null,null,null,null,"No",null,null,"Yes"]
[]
["BN",null,"Note: Environmental class C3 according to ISO/DIS 12944 for color Munsell 5.5B 5.5/1.25."]
["Surface",null,null,"C3",null,null,"C4",null,null,"C5 M H",null,null,null,"Other"]
["treatment"]
[null,null,"Colour"]
[]
["BO",null,"UBB Only"]
["Top section",null,null,"Cover mounting",null,null,null,null,null,"Yoke mounting on transformer's active part (Needed for bell type transformer)"]
[]
[]
[]
[]
[]
[]
[]
["BT",null,""]
["Supervisory devices",null,"Vertical distance H between the pressure relay device ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"m"]
[null,null,"and the oil level in the conservator"]
[null,null,"Note: One-way breather influences the set point level of our safety devices. "]
[null,null,"Add 4m to the real distance H if one-way breather is used."]
[null,null,"Note: One-way breather influence the set point level on our safety devices."]
[]
[null,null,"Note: Pressure relay and/or oil flow relay must be choosen."]
[null,null,"Pressure relay",null,null,null,null,null,null,null,null,null,"No",null,null,"Yes, double contacts"]
[null,null,"Oil flow relay",null,null,null,null,null,null,null,null,null,"No",null,null,"Yes"]
[null,null,"Pressure relief device",null,null,null,null,null,null,null,null,null,"No",null,null,"Yes, single contact"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Yes, double contacts"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Only flange for pressure relief device"]
[null,null,"Temperature relay",null,null,null,null,null,null,null,null,null,"No",null,null,"+115 degrees C"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"+105 degrees C"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-25 degrees C"]
[null,null,"Temperature sensor PT100 ",null,null,null,null,null,null,null,null,null,"No",null,null,"Yes"]
[null,null,"(Needed for TEC)",null,null,null,null,null,"Note: Not in combination with temperature switch"]
[]
["DA"]
["Documents",null,"Documents required in                    sets."]
[]
[null,null,"Note: More than 3 sets will be charged for!"]
[]
[]
["FR1",null,"All extras must be noted!"]
["Further "]
["requirements"]
["and revision"]
["specifications"]